**Section VI - Technical Specifications**

**Part II - Technical Data Sheets**

**table of contents**

|  |  |  |
| --- | --- | --- |
| **SECTION** | **DESCRIPTION** | **PAGE** |
| 1.0 | SPARE PARTS DATA | TDS-1 |

**PART II – TECHNICAL DATA SHEETS**

**SUPPLY AND DELIVERY OF CURRENT AND POTENTIAL TRANSFORMERS FOR METERING OF SIASI DPP**

**PR NO.S3-SIA21-028**

1. The Bidder shall complete this technical data sheet and submit the filled-up form with the technical proposal. The Bidder shall use continuation sheets as necessary for any other additional information keeping to the format shown herein or by reproducing the same.

2. NPC reserves the right to reject Bids without proper and/or specific data and information as required herein.

3. The data required are technical features and characteristics of the Equipment/Component/Parts to be provided by the bidder. Bidder’s proposal shall at least be equal or superior to the requirements specified by NPC.

1. **SPARE PARTS DATA**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **NPC REQUIREMENTS** | | | **SUPPLIER’S DATA** | |
| **PART NO.** | **QTY.** | | **PART NO.** | **QTY.** |
| 1 | CURRENT TRANSFORMER, POLE/OUTDOOR TYPE, 138 KV METERING, DUAL RATIO, 15 KV,  60 HZ, 2000/1500:5A |  | 1 | PC |  |  |
| 2 | POTENTIAL TRANSFORMER, POLE/OUTDOOR TYPE, 15 KVA METERING. 110 BIL, 8400/120 V,  0.3 ACCURACY, 60 HZ, RATIO 70:1, DOUBLE BUSHING |  | 1 | PC |  |  |

**Name of Bidder**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Signature of Bidder**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_