**Section VI - Technical Specifications**

**Part II - Technical Data Sheets**

**table of contents**

|  |  |  |
| --- | --- | --- |
| **SECTION** | **DESCRIPTION** | **PAGE** |
| 1.0 | SPARE PARTS DATA | TDS-1 |

**PART II – TECHNICAL DATA SHEETS**

**SUPPLY AND DELIVERY OF VARIOUS MECHANICAL SPARE PARTS FOR 275KW CUMMINS (NTAG855-G1B, SN: 4111293811) FOR PALIMBANG DPP**

1. The Bidder shall complete this technical data sheet and submit the filled-up form with the technical proposal. The Bidder shall use continuation sheets as necessary for any other additional information keeping to the format shown herein or by reproducing the same.

2. NPC reserves the right to reject Bids without proper and/or specific data and information as required herein.

3. The data required are technical features and characteristics of the Equipment/Component/Parts to be provided by the bidder. Bidder’s proposal shall at least be equal or superior to the requirements specified by NPC.

1. **SPARE PARTS DATA**

**MODEL NO.: NTAG855-G1B S/N: 4111293811**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **NPC REQUIREMENTS** | | | **SUPPLIER’S DATA** | |
| **PART NO.** | **QTY.** | | **PART NO.** | **QTY** |
| 1 | AIR FILTER | AF928M | 6 | PC |  |  |
| 2 | BEARING CONNECTION | 214950 | 2 | SET |  |  |
| 3 | BEARING, MAIN | AR7421 | 12 | PC |  |  |
| 4 | ELEMENT, FUEL FILTER |  | 30 | PC |  |  |
| 5 | INJECTOR | 3054233 | 12 | PC |  |  |
| 6 | LUBE OIL FILTER (OEM) | 3313283 | 30 | PC |  |  |
| 7 | PUSH ROD | 3046420 | 12 | PC |  |  |
| 8 | PUSH ROD | 3046430 | 12 | PC |  |  |
| 9 | RING SET, PISTON | 3801755 | 6 | SET |  |  |
| 10 | SET, UPPER ENGINE GASKET | 4024920 | 2 | PC |  |  |
| 11 | UPPER, ENGINE GASKET SET | 3801235 | 1 | SET |  |  |
| 12 | VALVE, EXHAUST | 145701 | 12 | PC |  |  |
| 13 | VALVE, INTAKE | 135957 | 12 | PC |  |  |

*“If the part number(s) indicated by the bidder under the “Supplier’s Data” column is not the same to the part number indicated under the “NPC's Requirement column”, the bidder will submit/attached the corresponding Service Bulletin issued by the OEM*/*Authorized Manufacturer or any documents that will support it, such as but not limited to the Catalogue/ Brochures/Parts Manual”. Provided that* “Certification from **\*Supplier** that the item(s) offered is the same as required in the Tender Documents”*must be submitted as post qualification requirement.*

Note:

**\*Supplier** refers to those mentioned/ covered under **a.2.4**

*TS- DRAWINGS AND DOCUMENTS TO BE SUBMITTED*

(*Section VI – Technical Specifications*)

(a.2.4 Distributor/Dealer, a Certificate of Authorized Distributorship/Dealership from the OEM or Authorized Manufacturer of OEM Parts or Licensee of the OEM.)

(The authority can be acquired from OEM, Manufacturer of OEM Parts or Licensee of the OEM.)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
| **Name of Bidder** |  | **Name and Signature of Authorized Representative** |  | **Signature** |